SECTION 273601 **-** TELEPHONE INTERCONNECTION CABINETS AND BOARDS

Edit title to suit if both not required.

1. GENERAL
   * + 1. SUBMITTALS
          1. Submittals for this section are subject to the re-evaluation fee identified in Article 4 of the General Conditions.
          2. Manufacturer’s installation instructions shall be provided along with product data.
          3. Submittals shall be provided in the order in which they are specified and tabbed (for combined submittals).
          4. Product Data:

For Telephone Interconnection Cabinets: Catalog sheets.

For Telephone Interconnection Boards: Plywood data.

1. PRODUCTS
   * + 1. TELEPHONE INTERCONNECTION CABINETS
          1. Code gage steel cabinets as produced by Square D Co., or Westinghouse Electric Corp., having:

Indicate type of mounting on the drawings.

Flush or surface type mounting cabinet as indicated on the drawings.

Hinged door (full size) and one piece trim.

Use paragraph below for standard institution lock (prisons, hospitals, office buildings, etc.).

Yale No. 511S lock with brass cylinder rosette, blind fastened from inside of door. Two No. 47 keys with each lock.

Use paragraph below if institution has special lock requirements. Word processing person: delete underlining before entering information.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Co. door locks, Cat. No. \_\_\_\_\_\_\_\_. Two keys with each lock to match existing keying system.

Use paragraph below where special locks are not required such as D.O.T. maintenance buildings or other small facilities.

Door lock. Two keys with each lock.

Indicate dimensions on the drawings.

Minimum dimensions as indicated on the drawings.

Plywood mounting board inside cabinet (full height and width of cabinet).

* + - 1. TELEPHONE INTERCONNECTION BOARDS
         1. Plywood Standard; Construction and Industrial Grades: U.S. Dept. of Commerce Product Standard PS-1.
         2. Plywood Species and Type: Any Group 1 species, A-D INT-APA, exterior glue; Plain Sliced face veneer.

1. EXECUTION
   * + 1. INSTALLATION
          1. Telephone Interconnection Cabinets: Install at locations indicated on the drawings.
          2. Telephone Interconnection Boards: Install plywood mounting board of size, and at locations indicated on drawings. Paint boards with one coat of primer and 2 coats of flat black enamel paint.

END OF SECTION 273601