SECTION 014217 - ABBREVIATIONS

This section is for use with architectural drawings for Department of Correctional Services projects.

1. GENERAL
	* + 1. DESCRIPTION
				1. This Section establishes the words and terms for abbreviations used on the Drawings.

| **ABBREVIATIONS** | **TERM** |
| --- | --- |
| **-A-** |
| AB | ANCHOR BOLT |
| ABRSV | ABRASIVE |
| ABUT | ABUTMENT |
| ABV | ABOVE |
| AC | AIR CONDITIONING |
| ACC | ACCESS |
| AC INSUL | ACOUSTICAL INSULATION |
| AC PLAS | ACOUSTICAL PLASTER |
| AC PNL | ACOUSTICAL PANEL |
| AC T | ACOUSTICAL TILE |
| AD | ACCESS DOOR |
| ADC | AUTOMATIC DOOR CLOSER |
| ADDL | ADDITIONAL |
| ADDM | ADDENDUM |
| ADH | ADHESIVE |
| ADJ | ADJUSTABLE |
| ADJC | ADJACENT |
| AFF | ABOVE FINISHED FLOOR |
| AFG | ABOVE FINISHED GRADE |
| AFL | ACCESS FLOOR |
| AFS | ABOVE FINISHED SLAB |
| AGGR | AGGREGATE |
| AHD | AHEAD |
| ALM | ALARM |
| ALT | ALTERNATE |
| ALT NO | ALTERNATE NUMBER |
| ALUM | ALUMINUM |
| AMT | AMOUNT |
| ANC | ANCHOR |
| ANOD | ANODIZED |
| ANT | ANTENNA |
| AP | ACCESS PANEL |
| APPROX | APPROXIMATE(LY) |
| APPX | APPENDIX |
| APT | APARTMENT |
| ARCH | ARCHITECT(URAL) |
| ARF | ABOVE RAISED FLOOR |
| ASB | ASBESTOS |
| ASB CEM | ASBESTOS CEMENT |
| ASC | ABOVE SUSPENDED CEILING |
| ASPH | ASPHALT |
| ASSN | ASSOCIATION |
| ASSY | ASSEMBLY |
| ATCH | ATTACHMENT |
| AUTO | AUTOMATIC |
| AV | AUDIO VISUAL |
| AVE | AVENUE |
| AVG | AVERAGE |
| AWG | AMERICAN WIRE GAGE |
|  |  |
| **-B-** |
| B | BATHROOM |
| B/ | BOTTOM OF |
| BBD | BULLETIN BOARD |
| BBR | BASEBOARD RADIATION |
| BD | BOARD |
| BEV | BEVEL |
| BI | BLACK IRON |
| BITUM | BITUMINOUS |
| BJT | BED JOINT |
| BL | BASE LINE |
| BLDG | BUILDING |
| BLK | BLOCK |
| BLKG | BLOCKING |
| BLST | BALLAST |
| BLVD | BOULEVARD |
| BLW | BELOW |
| BLW CLG | BELOW CEILING |
| BM | BENCH MARK |
| BOC | BOTTOM OF CURB |
| BOF | BOTTOM OF FOOTING |
| BOT | BOTTOM |
| BP | BASEPLATE |
| BR | BEDROOM |
| BRCG | BRACING |
| BRDG | BRIDGING |
| BRDG JST | BRIDGING JOIST |
| BRG | BEARING |
| BRG PL | BEARING PLATE |
| BRK | BRICK |
| BRKR | BREAKER |
| BRKT | BRACKET |
| BRS | BRASS |
| BRZ | BRONZE |
| B/S or BS | BOTH SIDES |
| BSHG | BUSHING |
| BSMT | BASEMENT |
| BTU | BRITISH THERMAL UNIT |
| BTUH | BRITISH THERMAL UNITS PER HOUR |
| BU | BUILT-UP |
| BUR | BUILT-UP ROOF |
| BVL | BEVEL(ED) |
| B/W | BOTH WAYS |
|  |  |
| **-C-** |
| CAB | CABINET |
| CAD | CADMIUM |
| CAP | CAPACITY |
| CARP | CARPET |
| CAT | CATALOG |
| CAV | CAVITY |
| CB | CATCH BASIN |
| CBORE | COUNTERBORE |
| C/C | CENTER TO CENTER |
| CCTV | CLOSED CIRCUIT TELEVISION |
| CEM | CEMENT |
| CEM PLAS | CEMENT PLASTER |
| CER | CERAMIC |
| CFLG | COUNTER FLASHING |
| CHAN | CHANNEL |
| CH BD | CHALKBOARD |
| CHFR | CHAMFER |
| CHL | CHLORINE |
| CHR PL | CHROME PLATED |
| CI | CAST IRON |
| CIP | CAST IRON PIPE |
| CIPC | CAST-IN-PLACE CONCRETE |
| CIR | CIRCLE |
| CIRC | CIRCULAR |
| CJ | CONTROL JOINT |
| CL | CENTER LINE |
| CLG | CEILING |
| CLG HT | CEILING HEIGHT |
| CLL | CONTRACT LIMIT LINE |
| CLO | CLOSET |
| CLOS | CLOSURE |
| CLP | CLAMP |
| CLR | CLEAR |
| CLRM | CLASSROOM |
| CMP | CORRUGATED METAL PIPE |
| CMPST | COMPOSITE |
| CMU | CONCRETE MASONRY UNIT |
| CNR | CORNER |
| CNTR | COUNTER |
| COEF | COEFFICIENT |
| COL | COLUMN |
| COLL | COLUMN LINE |
| COM | COMMON |
| COMB | COMBINATION |
| COMM | COMMUNICATION |
| COMP | COMPRESS(ED)(ION)(IBLE) |
| COMPL | COMPLETE |
| COMPT | COMPARTMENT |
| CONC | CONCRETE |
| CONC FL | CONCRETE FLOOR |
| CONF | CONFERENCE |
| CONN | CONNECTION |
| CONSTJ | CONSTRUCTION JOINT |
| CONSTR | CONSTRUCTION |
| CONT | CONTINUOUS(ATION) |
| CONTR | CONTRACT(OR) |
| COORD | COORDINATE |
| CORR | CORRIDOR |
| CORRG | CORRUGATED |
| COV | COVER |
| COV PL | COVER PLATE |
| CP | CONTROL PANEL |
| CPE | CORRUGATED POLYETHYLENE |
| CPR | COPPER |
| CPVC | CHLORINATED POLYVINYL CHLORIDE |
| CRCMF | CIRCUMFERENCE |
| CRS | COLD ROLLED STEEL |
| CS | CAST STONE |
| CSB | CONCRETE SPLASH BLOCK |
| CSG | CASING |
| CSK | COUNTERSUNK |
| CSMT | CASEMENT |
| CSP | CORRUGATED STEEL PIPE |
| CSWK | CASEWORK |
| CT | CERAMIC TILE |
| CTV | CABLE TELEVISION |
| CUB | CUBICLE |
| CUH | CABINET UNIT HEATER |
| CU YD | CUBIC YARD |
| CY | CUBIC YARD |
| CYL | CYLINDER |
|  |  |
| **-D-** |
| D | DEEP |
| D | DRAIN |
| DBC | DIAMETER BOLT CIRCLE |
| DBL ACT | DOUBLE ACTING |
| DBL GLZ | DOUBLE GLAZING |
| DEMO | DEMOLITION |
| DEPT | DEPARTMENT |
| DET | DETAIL |
| DF | DRINKING FOUNTAIN |
| DFR | DOOR FRAME |
| DH | DOUBLE HUNG |
| DI | DROP INLET |
| DIA | DIAMETER |
| DIAG | DIAGONAL |
| DIFF | DIFFERENCE |
| DIM | DIMENSION |
| DIN RM | DINING ROOM |
| DIP | DUCTILE IRON PIPE |
| DISP | DISPENSER |
| DIST | DISTANCE |
| DIV | DIVIDER |
| DJ | DOUBLE JOIST |
| DL | DEAD LOAD |
| DLV | DOOR LOUVER |
| DMH | DROP MANHOLE |
| DMPF | DAMPPROOFING |
| DMPR | DAMPER |
| DMT | DEMOUNTABLE |
| DN | DOWN |
| DO | DITTO |
| DR | DOOR |
| DRP | DRAINAGE PIPE |
| DRS | DRAINAGE STRUCTURE |
| DRW | DRY WELL |
| DS | DOWNSPOUT |
| DT | DRAIN TILE |
| DUPL | DUPLICATE |
| DVTL | DOVETAIL |
| DW | DISHWASHER |
| DWG | DRAWING |
| DWGS | DRAWINGS |
| DWL | DOWEL |
| DWR | DRAWER |
|  |  |
| **-E-** |
| E | EAST |
| EA | EACH |
| EB | EXPANSION BOLT |
| ECS | EPOXY COATING SYSTEM |
| EF | EACH FACE |
| EJ | EXPANSION JOINT |
| EL | ELEVATION |
| ELAST | ELASTOMERIC |
| ELEC | ELECTRICAL |
| ELEV | ELEVATOR |
| EMER | EMERGENCY |
| ENAM | ENAMEL |
| ENCL | ENCLOSURE |
| ENGR | ENGINEER |
| ENGY | ENERGY |
| ENTR | ENTRANCE |
| EP | ELECTRICAL PANEL |
| EPDM | ETHYLENE PROPYLENE DIENE MONOMER |
| EQ | EQUAL |
| EQUIP | EQUIPMENT |
| EQUIV | EQUIVALENT |
| ER | EPOXY RESIN |
| ERECT | ERECTION |
| ES | EXPOSED SURFACE |
| ESCAL | ESCALATOR |
| ESMT | EASEMENT |
| EST | ESTIMATE |
| ET | EPOXY TERRAZZO |
| EW | EACH WAY |
| EWC | ELECTRICAL WATER COOLER |
| EX | EXISTING |
| EXCA | EXCAVATE(ION) |
| EXH | EXHAUST |
| EXIST | EXISTING |
| EXP | EXPANSION |
| EXST GR | EXISTING GRADE |
| EXT | EXTERIOR |
|  |  |
| **-F-** |
| F/ | FACE OF |
| FAS | FASTEN |
| FB | FLAT BAR |
| FBD | FIBERBOARD |
| FBM | FEET BOARD MEASURE |
| FBO | FURNISHED BY OTHERS |
| FBRK | FACE BRICK |
| FC | FOOTCANDLE |
| FCO | FLOOR CLEANOUT |
| F/CONC | FACE OF CONCRETE |
| FD | FLOOR DRAIN |
| FDN | FOUNDATION |
| FDND | FOUNDATION DRAIN |
| FEC | FIRE EXTINGUISHER CABINET |
| FEM | FEMALE |
| FF | FACTORY FINISH |
| F/F | FACE TO FACE |
| FFE  | FINISH FLOOR ELEVATION |
| F/FIN | FACE OF FINISH |
| FH | FIRE HYDRANT |
| FGL | FIBERGLASS |
| FHC | FIRE HOSE CABINET |
| FHMS | FLAT HEAD MACHINE SCREW |
| FHP | FULL HEIGHT PARTITION |
| FHWS | FLAT HEAD WOOD SCREW |
| FIN | FINISH |
| FIN FL | FINISH FLOOR |
| FIN GR | FINISH GRADE |
| FJT | FLUSH JOINT |
| FL | FLASHING |
| FLDG | FOLDING |
| FLG | FLANGE |
| FLR | FLOOR (ING) |
| FLR FIN | FLOOR FINISH |
| FLR PL | FLOOR PLATE |
| FLUOR | FLUORESCENT |
| FM | FORCE MAIN |
| F/MAS | FACE OF MASONRY |
| FMBD | FORMBOARD |
| FN | FENCE |
| FND | FOUNDATION |
| FPL | FIREPLACE |
| FPM | FEET PER MINUTE |
| FPRF | FIREPROOFING |
| FPS | FEET PER SECOND |
| FR | FIRE RATING |
| FR MIR | FRAMED MIRROR |
| FR MIR/SHF | FRAMED MIRROR AND SHELF |
| FREQ | FREQUENCY |
| FRPB | FIBER REINFORCED PLASTIC BOARD |
| FRPP | FIBER REINFORCED PLASTIC PANELS |
| FRT | FRONT |
| FRZR | FREEZER |
| F/ST | FACE OF STUDS |
| FSTNR | FASTENER |
| FT | FOOT |
| FTG | FOOTING |
| FUR | FURNACE |
| FURN | FURNITURE |
| FURR | FURRING |
| FUT | FUTURE |
| FWC | FABRIC WALL COVERING |
| FXTR | FIXTURE |
|  |  |
|  |  |
| **-G-** |
| GA | GAGE |
| GAL | GALLON |
| GALV | GALVANIZED |
| GALVI | GALVANIZED IRON |
| GALVS | GALVANIZED STEEL |
| GB | GRAB BAR |
| GD | GUTTER DRAIN |
| GDR | GUARD RAIL |
| GEN | GENERATOR |
| GENL | GENERAL |
| GF | GROUND FACE |
| GL | GLASS |
| GL BLK | GLASS BLOCK |
| GLL | GRADING LIMIT LINE |
| GLU LAM | GLUE LAMINATED |
| GLZ | GLAZING |
| GLZ CMU | GLAZED CONCRETE MASONRY UNIT |
| GND | GROUND |
| GPM | GALLONS PER MINUTE |
| GPD | GALLONS PER DAY |
| GR | GRAD(E)(ING) |
| GRAN | GRANULAR |
| GR BM | GRADE BEAM |
| GRL | GRILLE |
| GR LN | GRADE LINE |
| GRTG | GRATING |
| GRV | GRAVITY ROOF VENTILATOR |
| GSKT | GASKET |
| GSS | GALVANIZED STEEL SHEET |
| GST | GLAZED STRUCTURAL TILE |
| GT | GLAZED TILE |
| GUT | GUTTER |
| GV | GATE VALVE |
| GVL | GRAVEL |
| GW | GUY WIRE |
| GYP | GYPSUM |
| GYP BD | GYPSUM BOARD |
| GYP PLAS | GYPSUM PLASTER |
|  |  |
| **-H-** |
| H | HIGH |
| HAGL | HEAT ABSORBING GLASS |
| HB | HOSE BIBB |
| HBGC | HIGH BUILD GLAZE COATING |
| HC | HOLLOW CORE |
| HCMU | HOLLOW CONCRETE MASONRY UNIT |
| HD | HEAVY DUTY |
| HDBD | HARDBOARD |
| HD JT | HEAD JOINT |
| HDNR | HARDENER |
| HDR | HEADER |
| HDWD | HARDWOOD |
| HDWE | HARDWARE |
| HEX | HEXAGONAL |
| HGR | HANGER |
| HGT | HEIGHT |
| HH | HANDHOLE |
| HNDRL | HANDRAIL |
| HO | HOLD-OPEN |
| HP | HORSE POWER |
| HORIZ | HORIZONTAL |
| HPT | HIGH POINT |
| HR | HOUR |
| HS | HIGH STRENGTH |
| HSB | HIGH STRENGTH BOLT |
| HT | HEIGHT |
| HTG | HEATING |
| HTR | HEATER |
| HVAC | HEATING, VENTILATING, AIR CONDITIONING |
| HWY | HIGHWAY |
| HYD | HYDRANT |
| HYDR | HYDRAULIC |
|  |  |
| **-I-** |
| ID | INSIDE DIAMETER |
| IJ | ISOLATION JOINT |
| INCAND | INCANDESCENT |
| INCL | INCLUDE(D)(ING) |
| INL | INLET |
| INSTL | INSTALLATION |
| INSUL | INSULATION |
| INSUL PNL | INSULATED PANEL |
| INT | INTERIOR |
| INTLK | INTERLOCK |
| INV | INVERT |
| INV EL | INVERT ELEVATION |
| ISO | ISOMETRIC |
|  |  |
| **-J-** |
| JAN | JANITOR |
| JC | JANITOR’S CLOSET |
| JF | JOINT FILLER |
| JST | JOIST |
| JT | JOINT |
|  |  |
| **-K-** |
| K | KIP(1000 LB) |
| KB | KNEE BRACE |
| KCP | KEENE’S CEMENT PLASTER |
| KD | KILN DRIED |
| KIP FT | ONE THOUSAND FOOT POUNDS |
| KIT | KITCHEN |
| KLF | KIPS PER LINEAR FOOT |
| KO | KNOCKOUT |
| KOP | KNOCKOUT PANEL |
| KPL | KICK PLATE |
| KSF | KIPS PER SQUARE FOOT |
| KSI | KIPS PER SQUARE INCH |
| KWY | KEYWAY |
|  |  |
| **-L-** |
| L | LENGTH |
| LAB | LABORATORY |
| LAD | LADDER |
| LAM | LAMINATION |
| LAU | LAUNDRY |
| LAV | LAVATORY |
| LB | POUND |
| LBL | LABEL |
| LBR | LUMBER |
| LBSN | LEACHING BASIN |
| LCMU | LIGHTWEIGHT CONCRETE MASONRY UNIT |
| LD BRG | LOAD BEARING |
| LDG | LANDING |
| LF | LINEAR FOOT |
| LG or LONG | LENGTH |
| LH | LEFT HAND |
| LHR | LEFT HAND REVERSE |
| LIB | LIBRARY |
| LIN | LINEAR |
| LKR | LOCKER |
| LKR RM | LOCKER ROOM |
| LL | LIVE LOAD |
| LLH | LONG LEG HORIZONTAL |
| LLV | LONG LEG VERTICAL |
| LMS | LIMESTONE |
| LNTL | LINTEL |
| LOC | LOCATION |
| LONG | LONGITUDINAL |
| LP | LIGHTPROOF |
| LPT | LOW POINT |
| LR | LIVING ROOM |
| LRG | LARGE |
| LS | LOUDSPEAKER |
| LT | LIGHT |
| LTG | LIGHTING |
| LTG PNL | LIGHTING PANEL |
| LT WT | LIGHTWEIGHT |
| LVL | LEVEL(ER) |
| LVR | LOUVER |
| LWC | LIGHTWEIGHT CONCRETE |
| LW PLAS | LIGHTWEIGHT PLASTER |
|  |  |
| **-M-** |
| MACH RM | MACHINE ROOM |
| MAINT | MAINTENANCE |
| MALI | MALLEABLE IRON |
| MANUF | MANUFACTURER |
| MARB | MARBLE |
| MAS | MASONRY |
| MATL | MATERIAL |
| MATV | MASTER ANTENNA TELEVISION SYSTEM |
| MAX | MAXIMUM |
| MB | MACHINE BOLT |
| MBF | THOUSAND BOARD FEET |
| MBH | MOP/BROOM HOLDER |
| MDO | MEDIUM DENSITY OVERLAID |
| MECH | MECHANICAL |
| MED | MEDIUM |
| MEMB | MEMBRANE |
| MET | METAL |
| METB | METAL BASE |
| MEZZ | MEZZANINE |
| MFG | MANUFACTURER |
| MFG | MANUFACTURING |
| MH | MANHOLE |
| MI | MILE |
| MIN | MINIMUM |
| MISC | MISCELLANEOUS |
| MJ | MECHANICAL JOINT |
| ML | METAL LATH |
| MLDG | MOLDING |
| MLWK | MILL WORK |
| MO | MASONRY OPENING |
| MOD | MODULE(AR) |
| MON | MONUMENT |
| MR | MOISTURE RESISTANT |
| MSB | MOP SERVICE BASIN |
| MT | MOUNT(ING) |
| MTD | MOUNTED |
| MTG | MEETING |
| MTL | METAL |
| MTR | MORTAR |
| MULL | MULLION |
| MULT | MULTIPLE |
| MVBL | MOVABLE |
|  |  |
| **-N-** |
| N | NORTH |
| NA | NOT APPLICABLE |
| NAT | NATURAL |
| NC | NOISE CRITERIA |
| NEG | NEGATIVE |
| NIC | NOT IN CONTRACT |
| NKL | NICKEL |
| NO | NUMBER |
| NOM | NOMINAL |
| NPL | NAMEPLATE |
| NPT | NATIONAL PIPE THREAD |
| NR | NOISE REDUCTION |
| NRC | NOISE REDUCTION COEFFICIENT |
| NTS | NOT TO SCALE |
|  |  |
| **-O-** |
| OA | OVERALL |
| OBS | OBSCURE |
| OC | ON CENTER |
| OD | OUTSIDE DIAMETER |
| OF | OUTSIDE FACE |
| OFF | OFFICE |
| OHGW | OVERHEAD GUY WIRE |
| OHMS | OVAL HEAD MACHINE SCREW |
| OHWS | OVAL HEAD WOOD SCREW |
| OJ | OPEN WEB JOISTS |
| O/O | OUT TO OUT |
| OP | OPAQUE |
| OPNG | OPENING |
| OPP | OPPOSITE |
| OPPH | OPPOSITE HAND |
| OPT | OPTIONAL |
| ORD | OVERFLOW ROOF DRAIN |
| ORIG | ORIGINAL |
| OS&Y | OUTSIDE SCREW AND YOKE |
| OVFL | OVERFLOW |
| OVHD | OVERHEAD |
| OZ | OUNCE |
|  |  |
| **-P-** |
| PA | PUBLIC ADDRESS |
| PAR | PARALLEL |
| PARG | PARGING |
| PBD | PARTICLEBOARD |
| PC | POINT OF CURVATURE |
| PCC | POINT OF COMPOUND CURVATURE |
| PCF | POUNDS PER CUBIC FOOT |
| PCP | PORTLAND CEMENT PLASTER |
| PERF | PERFORATED |
| PERIM | PERIMETER |
| PERM | PERMANENT |
| PERP | PERPENDICULAR |
| PGBD | PEGBOARD |
| PHS | PHILLIP’S HEAD SCREW |
| PI | POINT OF INTERSECTION |
| PIV | POST INDICATOR VALVE |
| PKG | PACKAGE |
| PL | PLATE |
| PLAM | PLASTIC LAMINATE |
| PLAS | PLASTER |
| PLAT | PLATFORM |
| PLBG | PLUMBING |
| PLF | POUNDS PER LINEAR FOOT |
| PLYWD | PLYWOOD |
| PNL | PANEL |
| PNT | PAINT |
| PO | PLUGGED OUTLET |
| POB | POINT OF BEGINNING |
| POC | POINT ON CURVE |
| POL | POLISHED |
| POLY | POLYETHYLENE |
| PORT | PORTABLE |
| POS | POSITIVE |
| POT | POINT OF TANGENCY |
| PP | PLASTIC PIPE |
| PR | PAIR |
| PRC | POINT OF REVERSE CURVATURE |
| PRCST | PRECAST |
| PREFAB | PREFABRICATED |
| PREFIN | PREFINISHED |
| PREGV | PRESSURE REGULATING VALVE |
| PRELIM | PRELIMINARY |
| PREP | PREPARATION |
| PRKG | PARKING |
| PROJ | PROJECT |
| PROP | PROPERTY |
| PROP LN | PROPERTY LINE |
| PRV | PRESSURE REDUCING VALVE |
| PS | PUMPING STATION |
| PS CONC | PRESTRESSED CONCRETE |
| PSF | POUNDS PER SQUARE FOOT |
| PSI | POUNDS PER SQUARE INCH |
| PT | POINT |
| PT | PRESSURE TREATED |
| PTD | PAPER TOWEL DISPENSER |
| PTN | PARTITION |
| PTR | PAPER TOWEL RECEPTACLE |
| PV | PAVED |
| PVC | POLYVINYL CHLORIDE |
| PVG | PAVING |
| PVMT | PAVEMENT |
| PWR | POWER |
|  |  |
| **-Q-** |
| QT | QUARRY TILE |
| QTY | QUANTITY |
| QUAL | QUALITY |
|  |  |
| **-R-** |
| R | THERMAL RESISTANCE |
| RI | RISER |
| RAD | RADIUS |
| RADN | RADIATION |
| RBR | RUBBER |
| RC | REINFORCED CONCRETE |
| RCP | REINFORCED CONCRETE PIPE |
| RD | ROOF DRAIN |
| REC | RECESSED |
| RECD | RECEIVED |
| RECT | RECTANGULAR |
| REF | REFERENCE |
| REFL | REFLECTOR |
| REFR | REFRIGERATOR |
| REG | REGISTER |
| REINF | REINFORCE(D)(ING)(MENT) |
| REM | REMOVEABLE |
| REP | REPRESENTATIVE |
| REPRO | REPRODUCE |
| REQD | REQUIRED |
| RESIL | RESILIENT |
| REV | REVISED, REVISION |
| RFG | ROOFING |
| RH | RIGHT HAND |
| RHMS SCREW | ROUND HEAD MACHINE |
| RHR | RIGHT HAND REVERSE |
| RHWS | ROUND HEAD WOOD SCREW |
| RLG | RAILING |
| RM | ROOM |
| RND | ROUND |
| RO | ROUGH OPENING |
| ROW | RIGHT OF WAY |
| RPM | REVOLUTIONS PER MINUTE |
| RS | RESILIENT SHEET |
| RV | ROOF VENT |
| RVS | REVERSE |
| RVT | RIVETED |
|  |  |
| **-S-** |
| S | SOUTH |
| SAN | SANITARY |
| SB | SPLASH BLOCK |
| SC | SOLID CORE |
| SCHED | SCHEDULE |
| SCMU | SOLID CONCRETE MASONRY UNIT |
| SCR | SHOWER CURTAIN ROD |
| SCRN | SCREEN |
| SCT | STRUCTURAL CLAY TILE |
| SD | SOAP DISPENSER  |
| SDL | SADDLE |
| SECT | SECTION |
| SF | SQUARE FEET |
| SFT | STRUCTURAL FACING TILE |
| SGL | SINGLE SHOWER |
| SHT | SHEET(ING) |
| SHTHG | SHEATHING |
| SHV | SHELVES(ING) |
| SIM | SIMILAR |
| SJ | SCORED JOINT |
| SK | SINK |
| SLP | SLOPE |
| SLV | SLEEVE |
| SM | SURFACE MOUNTED |
| SNT | SEALANT |
| SPEC | SPECIFICATION |
| SPKR | SPEAKER |
| SPLY | SUPPLY |
| SPRT | SUPPORT |
| SQ | SQUARE |
| SQ FT | SQUARE FOOT |
| SQ IN | SQUARE INCH |
| SQ YD | SQUARE YARD |
| SS | SANITARY SEWER |
| SS | STAINLESS STEEL |
| SSK | SERVICE SINK |
| SST | STAINLESS STEEL |
| ST | STREET |
| STA | STATION |
| STAG | STAGGERED |
| STC | SOUND TRANSMISSION CLASS |
| STD | STANDARD |
| STG | SEATING |
| STIF | STIFFENER |
| STL | STEEL |
| STL JST | STEEL JOIST |
| STL PL | STEEL PLATE |
| STOR | STORAGE |
| STR | STRAIGHT |
| STRUCT | STRUCTURAL |
| STRUCT STL | STRUCTURAL STEEL |
| SURF | SURFACE |
| SURV | SURVEY |
| SUSP | SUSPENDED |
| SUSP CLG | SUSPENDED CEILING |
| SW | SIDEWALK |
| SWBD | SWITCHBOARD |
| SWR | SEWER |
| SYM | SYMBOL |
| SYMM | SYMMETRICAL |
| SYNTH | SYNTHETIC |
| SYS | SYSTEM |
|  |  |
| **-T-** |
| T | TREAD |
| T/ | TOP OF |
| TB | TOWEL BAR |
| T&B | TOP AND BOTTOM |
| T/BM | TOP OF BEAM |
| T/CONC | TOP OF CONCRETE |
| TD | TRENCH DRAIN |
| TDH | TOTAL DYNAMIC HEAD |
| TE | TOP ELEVATION |
| TEL | TELEPHONE |
| TEMP | TEMPORARY |
| TERR | TERRAZZO |
| TF | TOP OF FRAME ELEVATION |
| T/FF | TOP OF FINISH FLOOR |
| T/FTG | TOP OF FOOTING |
| T&B | TOP AND BOTTOM |
| T&G | TONGUE AND GROOVE |
| THBLK | THRUST BLOCK |
| THK | THICKNESS |
| THRES | THRESHOLD |
| THRU | THROUGH |
| TI | TAPERED INSULATION |
| T/JST | TOP OF JOIST |
| TK BD | TACKBOARD |
| TKS | TACKSTRIP |
| TLT | TOILET |
| TMPD | TEMPERED |
| TMPD GL | TEMPERED GLASS |
| TOC | TOP OF CURB |
| TOF | TOP OF FOOTING |
| TOT | TOTAL |
| TOW | TOP OF WALL |
| TPTN | TOILET PARTITION |
| TS | TUBE STEEL |
| T/SL | TOP OF SLAB |
| T/STL | TOP OF STEEL |
| TV | TELEVISION |
| T/W | TOP OF WALL |
| TYP | TYPICAL |
|  |  |
| **-U-** |
| UC | UNDERCUT |
| UCR | UNDER COUNTER REFRIGERATOR |
| UG | UNDER GROUND |
| UL | UNDERWRITERS LABEL |
| UNEX | UNEXCAVATED |
| UNFIN | UNFINISHED |
| UNIF | UNIFORM |
| UON | UNLESS OTHERWISE NOTED |
| UNO | UNLESS NOTED OTHERWISE |
| URIN | URINAL |
| UTIL | UTILITY |
| **-V-** |
| VA | VALVE |
| VAP | VAPOR |
| VAP PRF | VAPOR PROOF |
| VAR | VARNISH |
| VB | VAPOR BARRIER |
| VCP | VITRIFIED CLAY PIPE |
| VCT | VINYL COMPOSITION TILE |
| VEH | VEHICLE |
| VENT | VENTILATOR |
| VERM | VERMICULITE |
| VERT | VERTICAL |
| VEST | VESTIBULE |
| VFAT | VINYL FACED ACOUSTIC TILE |
| VIN | VINYL |
| VIT | VITREOUS |
| VNR | VENEER |
| VT | VINYL TILE |
| VTP | VITRIFIED TILE PIPE |
| VWC | VINYL WALL COVERING |
|  |  |
| **-W-** |
| W | WEST |
| W/ | WITH |
| WC | WATER CLOSET |
| WD | WOOD |
| WDW | WINDOW |
| WF | WIDE FLANGE |
| WFR | WAFER |
| WGL | WIRE GLASS |
| WH | WALL HUNG |
| WHYD | WALL HYDRANT |
| WHSE | WAREHOUSE |
| WI | WROUGHT IRON |
| WL | WIND LOAD |
| WLD | WELDED |
| WLS | WALL LOUVER AND SCREEN |
| W\O | WITHOUT |
| WP | WATERPROOF |
| WPT | WORKING POINT |
| WR | WATER RESISTANT |
| WS | WEATHERSTRIPPING |
| WSCT | WAINSCOT |
| WSURF | WATER SURFACE |
| WT | WEIGHT |
| WTR | WATER |
| WTRPRF | WATERPROOFING |
| W/W | WALL TO WALL |
| WWM | WELDED WIRE MESH |
| WWF | WELDED WIRE FABRIC |
|  |  |
| **-X-** |
| X SECT | CROSS SECTION |
|  |  |
| **-Y-** |
| YD | YARD |
| YDD | YARD DRAIN |
| YHYD | YARD HYDRANT |
|  |  |

1. PRODUCTS (Not Used)
2. EXECUTION (Not Used)

END OF SECTION 014217